# For more options and information see
# http://rpf.io/configtxtreadme
# Some settings may impact device functionality. See link above for details

# uncomment if you get no picture on HDMI for a default "safe" mode
#hdmi_safe=1

# uncomment this if your display has a black border of unused pixels visible
# and your display can output without overscan
#disable_overscan=1

# uncomment the following to adjust overscan. Use positive numbers if console
# goes off screen, and negative if there is too much border
#overscan_left=16
#overscan_right=16
#overscan_top=16
#overscan_bottom=16

# uncomment to force a console size. By default it will be display's size minus
# overscan.
#framebuffer_width=1280
#framebuffer_height=720

# uncomment if hdmi display is not detected and composite is being output
#hdmi_force_hotplug=1

# uncomment to force a specific HDMI mode (this will force VGA)
#hdmi_group=1
#hdmi_mode=1

# uncomment to force a HDMI mode rather than DVI. This can make audio work in
# DMT (computer monitor) modes
#hdmi_drive=2

# uncomment to increase signal to HDMI, if you have interference, blanking, or
# no display
#config_hdmi_boost=4

# uncomment for composite PAL
#sdtv_mode=2

#uncomment to overclock the arm. 700 MHz is the default.
#arm_freq=800

# Uncomment some or all of these to enable the optional hardware interfaces
#dtparam=i2c_arm=on
#dtparam=i2s=on
#dtparam=spi=on

# Uncomment this to enable the lirc-rpi module
#dtoverlay=lirc-rpi

# Additional overlays and parameters are documented /boot/overlays/README

# Enable audio (loads snd_bcm2835)
dtparam=audio=on
gpu_mem_256=128
gpu_mem_512=256
gpu_mem_1024=256
overscan_scale=1

# add this entire file to your /boot/config.txt
#
# BEGIN FREEPLAY MODS
framebuffer_width=320
framebuffer_height=240
hdmi_force_hotplug=1   #these HDMI lines will try to set up 1024x768 (you can remove them if you have problems playing via HDMI)
HDMI_FORCE_MODE=1
hdmi_group=2
hdmi_mode=16
hdmi_drive=1           #Normal DVI mode (No sound) (2 for HDMI with sound)
dtparam=spi=on
dtparam=audio=on
dtoverlay=waveshare32b,speed=80000000,fps=60,rotate=270
[pi0]
#Freeplay Zero
dtoverlay=audremap,swap_lr=off
[pi3]
#Freeplay CM3
dtoverlay=audremap,swap_lr=on
[pi2]
#Sometimes we test with Pi2
dtoverlay=audremap,swap_lr=on
[all]
dtoverlay=gpio-poweroff,gpiopin=21,active_low
# Disable the ACT LED on the Pi Zero.
dtparam=act_led_trigger=none
dtparam=act_led_activelow=on
audio_pwm_mode=2
dtparam=watchdog=on	# Enabling watchdog.
# remove # from following 2 lines to turn wifi and bluetooth off (if not needed, can Speed Up Pi Zero W)
#dtoverlay=pi3-disable-wifi
#dtoverlay=pi3-disable-bt
# END FREEPLAY MODS
